**SpeedAC iQ – Duplex Net Weigher V2.5.0b changes summary:**

***IMPORTANT: Databases from the previous versions are not compatible***

**Improvements/New features:**

* Parameter BSF Bulk Off delay is added in Machine parameter. This parameter is used to add a delay after the bulk cutoff is reached, before putting the bulk signal Off. It’s only used for the BSF feeder type.

**Fixes:**