**SpeedAC iQ – In Process V3.0.5 changes summary:**

***IMPORTANT: Databases from the previous versions are compatible***

**Fixes:**

* Correction of Cut Offs Values is fixed (Standard & not MP.AutoSaveCorr);
* PLC Write command is fixed;
* Max feed rate fixed to 999,999kg/h;